UG_IO SimSys 2D Node, Grid, and Function File Types

    File Type Suffix and Description
    ________________________________________________________________________________

    .snode2d
    --------
    SNODE 2D source node data file.
    An SNODE file contains a list of node coordinates and spacing function.
    This file type uses a fixed file format that is either a standard ASCII file
    format or a binary format specific to the file type.

    .mnode2d
    --------
    MNODE 2D metric source node data file.
    A MNODE file contains a list of node coordinates and symmetric metric.
    This file type uses a fixed file format that is either a standard ASCII file
    format or a binary format specific to the file type.

    .bedge
    ------
    BEDGE 2D B-Edge Grid File
    A BEDGE file contains a boundary edge grid.
    This file type uses a fixed file format that is either a standard ASCII file
    format or a binary format specific to the file type.
    This file type may only be used for input files.

    .fgrid
    ------
    FGRID 2D unstructured grid file.
    An FGRID file contains a boundary edge grid and (optionally) a tria face planar
    grid. The FGRID 2D file type is derived from the 3D FGRID file type.
    Differences include additional boundary edge grid data, no volume elements, and
    all z-coordinates are zero.

    .mesh
    -----
    MESH 2D unstructured grid file.
    A MESH file contains a boundary edge grid and (optionally) a tria/quad face
    planar grid.
    This file type is supported by the Gamma Project of INRIA.
    This file type uses a fixed file format that is either a standard ASCII file
    format or a binary format specific to the file type.

    .meshb
    ------
    Binary MESH 2D unstructured grid file.
    A MESH file contains a boundary edge grid and (optionally) a tria/quad face
    planar grid.
    This file type is supported by the Gamma Project of INRIA.
    This file type uses a fixed file format that is either a standard ASCII file
    format or a binary format specific to the file type.

    .ugrid
    ------
    UGRID 2D Unstructured Grid File
    A UGRID file contains a boundary edge grid and (optionally) a mixed tria/quad
    face planar grid. The UGRID 2D file type is derived from the 3D UGRID file
    type. Differences include additional boundary edge grid data, no volume
    elements, and all z-coordinates are zero.

    .ufunc
    ------
    UFUNC 2D function file.
    A UFUNC file contains field function data (scalar and/or vector).
    This file type can use socket or TMP file mode if a C binary double file format
    is also used.

    .sfunc
    ------
    SFUNC 2D function file.
    An SFUNC file contains field function data (scalar, vector, matrix, and/or
    symmetric metric).
    This file type can use socket or TMP file mode if a C binary double file format
    is also used.

    .sol
    ----
    MESH SOL 2D unstructured function file.
    A MESH SOL file contains field function data (scalar, vector, matrix, and/or
    symmetric metric). This file type is supported by the Gamma Project of INRIA.
    This file type uses a fixed file format that is either a standard ASCII file
    format or a binary format specific to the file type.

    .solb
    -----
    Binary MESH SOL 2D unstructured function file.
    A MESH SOL file contains field function data (scalar, vector, matrix, and/or
    symmetric metric). This file type is supported by the Gamma Project of INRIA.
    This file type uses a fixed file format that is either a standard ASCII file
    format or a binary format specific to the file type.

Details on the specific file types are available in the UG_IO SimSys 2D Node, Grid, and Function File Types section for the standard 32-bit int version. Note that only those listed above are applicable with the 64-bit version.

UG_IO SimSys Files Home

ugc_l version 7.5.16
Last Updated Wed Feb 22 22:13:24 CST 2017